How to install the software ?

a) Run "SETUP.exe" in file named "DataRecieve"
b) The step of installation is running automaticlly
c) You will get a "shortcut" named "DataReceiver" in your "Program File"
d) Run this "shortcut" named "DataReceiver", the software will be OK.

How to transfer the data stored  to PC?

a) After run the step above, you will get a software window on the screen of your PC
b) Select the "Options", you must change the serial baudrate to 2400 bps
c) Connect the gauge to PC with the transfer cable
d) Power on the gauge. Select the "Options", run the "Activate Ports", you will get the effective port 
   of your computer and confirm it
e) The "Receive State" on the left indicates the state of transmission, "Opened" means the PC is ready to receive
   the data you transfer, "Closed" means the connection is closed
f) You can transfer the data in gauge to PC according to the step described in your manual
g) You can save the data transfered to PC as *.xls *.doc and *.txt after your transmission

   Notice: some unjustifiable symbol will display in the step of transmission, you should delet them before you save 
the data.

